|  |  |  |  |
| --- | --- | --- | --- |
| **SAIPRO INDUSTRIES PVT LTD** | | | |
| **PREVENTIVE MAINTANANCE CHECKLIST - AHU** | | | |
| **FORMAT NO.** | | **SIPL/SOP/EN/04-F01** | |
| **EQUIPMENT NO.** | |  | |
| **LOCATION** | |  | |
| **DATE** | |  | |
| **SR. NO** | **PARAMETERS TO BE CHECK** | **STATUS** | **ACTIONS TO BE TAKENS** |
| 1 | CHECK THE MAIN SWITCH | ON/OFF |  |
| 2 | CHECK THE CONDITION OF "V" BELT | OK/NOT OK/NA |  |
| 3 | CHECK BELT TENSION | OK/NOT OK |  |
| 4 | CHECK FOUNDATION BELD OF MOTOR | OK/ LOOSE |  |
| 5 | CHECK BALENCING OF BLOWER | OK/NOT OK/NA |  |
| 6 | CHECK ALL POWER AND ELECTRICAL CONNECTIONS | OK/ LOOSE |  |
| 7 | CHECK THE DRAIN LINE OF DRAIN TRAY | CLEANED / DUSTY |  |
| 8 | CHECK THE FILTER CONDITION | CLEANED / DUSTY |  |
| 9 | CHECK FOR AIR LEAKADGE ON ALL THE JOINTS & DOORS | OK/LEAKAGE |  |
| 10 | CHECK MANOMETER READINGS (IF APPLICABLE) & IF  PRESSURE DIFFRENCIAL READINGS ( IFAPPLICABLE | OK/NOT OK/NA |  |
| 11 | CHECK TEMP SENSOR & HUMIDITY SENSOR | OK/NOT OK/NA |  |
|  | | | |
| **DONE BY CHECKED BY** | | | |